**OKY4005-1**

**Product Name:**LCD 1602 LCD 16x2 Serial Lcd Display Module For Uno R3 Mega 2560

**Product Module：**OKY4005-1

**Product Description:**

1.This is another great yellow backlight LCD display. As the pin resources of Arduino controller is limited, your project may be not able to use normal LCD shield after connected with a certain quantity of sensors or SD card. However, with this I2C interface LCD module, you will be able to realize data display via only 2 wires. If you already has I2C devices in your project, this LCD module actually cost no more resources at all. It is fantastic for Arduino based project.

2.I2C Address: 0x27.

3.Pin Definition : VCC、GND、SDA、SCL.

4.Back lit (Green with white char color).

5.Supply voltage: 5V.

6.Size : 27.7mm×42.6mm.

7.Contrast Adjust : Through Potentiometer.

8.Only employ two I/O interface.

**Package Included**

|  |  |
| --- | --- |
| Packing List | Qty |
| LCD 1602 LCD 16x2 Serial Lcd Display Module  | 1 |